#
SIDE PROTECTOR REMOVAL

id091600801100

1. Pry the side protector end 20-30 mm {0.8-1.1 in} using a flathead screwdriver or a razor.

  Warning

  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

  Note

  • The side protector is installed with double-sided adhesive tape. If the side protector is difficult to remove, warm the double-sided adhesive tape using a hot air blower.

2. Pull the side protector outward, then remove it from the body.