#
PARAMETER IDENTIFICATION (PID) DATA MONITORING FUNCTION [FN4A-EL]

id0502a1100700
• The PID mode allows access to certain data values, analog and digital input and output, calculated values, and system states information.

Monitor Item Table

Display on the tester | Definition | Unit/Condition | PCM terminal
--- | --- | --- | ---
GEAR | Gear commanded by module | 1/2/3/4 | 1AJ 1AR 1AZ 1BD 1BH
LINEDES | Target modifier pressure | KPa | psi | 1AF 1AV
LPS | Pressure control solenoid control signal in PCM | A | 1AF 1AV
SSA/SS1 | Shift solenoid A control signal in PCM | % | 1AZ
SSB/SS2 | Shift solenoid B control signal in PCM | % | 1BH
SSC/SS3 | Shift solenoid C control signal in PCM | % | 1BD
TCS | HOLD switch | On/Off | 1AQ
TEST | - | On/Off | -
TFT | ATF temperature | °C | °F | 1AN 1AU
TFTV | ATF temperature signal voltage | V | 1AN 1AU
THOP | TP signal in PCM | % | 2AA
TP | TP signal voltage | V | % | 2AA
TR | TR switch signal | R/N/D/S/L | 1X
TR_SENS | TR switch signal voltage | V | 1X
TSS | Input/turbine speed | RPM | 1K 1O
VPWR | Battery positive voltage | V | 1AX 1BF 1BG
VSS | Vehicle speed | KPH | MPH | 1AY 1BC