#
KNOCK SENSOR REMOVAL/INSTALLATION

id014000802900

1. Disconnect the negative battery cable.

2. Disconnect the knock sensor connector.

3. Remove the following part for easier access.

  • Intake manifold (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITHOUT WU-TWC], INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].)

4. Using the SST, remove the knock sensor.

5. Install in the reverse order of removal.

Tightening torque

  19.6-34.3 N·m {2.0-3.4 kgf·m, 15-25 ft·lbf}