#
GENERAL PROCEDURES (BRAKE)

ADA0410id041000800100

## Wheel And Tire Removal/Installation

1. When installing a wheel, tighten the wheel nuts in opposing diagonal order to the following torque.

Tightening torque

  88.2-117.6 N·m {9.00-11.99 kgf·m, 65.06-86.73 ft·lbf}

## Brake Lines Disconnection/Connection

1. If any brake line has been disconnected anytime during the procedures, add brake fluid, bleed the brakes, and inspect for leakage after the procedure has been completed.

  Caution

  • Brake fluid will damage painted surfaces. Be careful not to get any on painted surface. If brake fluid gets on painted surfaces, wipe it off immediately.

## Brake pipe flare nut tightening

1. Tighten the brake pipe flare nut using the SST (49 0259 770B) or any commercially available flare nut wrench.

## ABS component operations

1. Make sure that there are no DTCs in the ABS memory after working on ABS components. If there are any codes in the memory, erase them.