#
CAMSHAFT POSITION (CMP) SENSOR REMOVAL/INSTALLATION

id014000801500

  Caution

  • When replacing the CMP sensor, make sure there is no foreign material on it such as metal shavings. If it is installed with foreign material, the sensor output signal will malfunction resulting from fluctuation in magnetic flux and cause a deterioration in engine control.

1. Disconnect the negative battery cable.

2. Disconnect the CMP sensor connector.

3. Remove the CMP sensor installation bolt.

4. Remove the CMP sensor.

5. Verify that the O-ring is not damaged.

  • If there is any damage, replace the CMP sensor.

6. Apply a small amount of clean oil to the O-ring and the head cover.

7. Install in the reverse order of removal.

Tightening torque

  7.8-10.8 N·m {0.8-1.1 kgf·m, 5.8-7.9 ft·lbf}