#
PRIMARY SHAFT COMPONENTS DISASSEMBLY

B3E051517201102

1. Disassemble in the order indicated in the table.

1 | Bearing (4th gear end) (See Bearing (4th Gear End) Disassembly Note.)
2 | 4th gear
3 | 4th synchronizer ring
4 | Retaining ring
5 | 3rd/4th clutch hub component (See 3rd/4th Clutch Hub Component, 3rd Synchronizer Ring and 3rd Gear Disassembly Note.)
6 | 3rd synchronizer ring (See 3rd/4th Clutch Hub Component, 3rd Synchronizer Ring and 3rd Gear Disassembly Note.)
7 | 3rd gear (See 3rd/4th Clutch Hub Component, 3rd Synchronizer Ring and 3rd Gear Disassembly Note.)
8 | Bearing (primary shaft end) (See Bearing (Primary Shaft End) Disassembly Note.)
9 | Primary shaft gear
10 | Synchronizer key spring
11 | 3rd/4th clutch hub sleeve
12 | Synchronizer key
13 | 3rd/4th clutch hub

## Bearing (4th Gear End) Disassembly Note

1. Remove the bearing using the SST.

## 3rd/4th Clutch Hub Component, 3rd Synchronizer Ring and 3rd Gear Disassembly Note

1. Remove the retaining ring.

2. Remove the 3rd/4th clutch hub component, 3rd synchronizer ring, and 3rd gear using the SST.

## Bearing (Primary Shaft End) Disassembly Note

1. Remove the bearing using the SST.

  Caution

  • Use protective plates in the vise to prevent damage to the primary shaft gear.