#
AFTER REPAIR PROCEDURE

CDA011400000W02

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, always complete the "Fuel Line Inspection".

## Fuel Leakage Inspection

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes.To prevent this, complete the following inspection with the engine stopped.

1. Remove the fuel pump relay.

  Caution

  • Short the specified terminal as shortening the wrong terminal of the main fuse block may cause a malfunction.

2. Using a jumper wire, short fuel pump relay terminals C and D and start the fuel pump.

3. Verify that there is no fuel leakage from the pressurized parts.

  • If there is leakage, replace the fuel hoses and clips.
  • If there is damage on the seal on the fuel pipe side, replace the fuel pipe.

Fuel leakage

  There shall be no leakage after 5 min.

4. After reinstallation, repeat step 2-3 in the fuel leakage inspection.