CYLINDER HEAD INSPECTION

id011000507100

1. Carry out the color contrast penetrate examination on the cylinder head surface.

  • If there is a crack, replace the cylinder head.

2. Measure the combustion chamber side of the cylinder head for distortion in six directions as shown in the figure using a straight edge and feeler gauge.

bezeze00000029

  • If it exceeds the maximum specification, replace the cylinder head. Do not attempt to repair the cylinder head by milling or grinding.

  Maximum distortion

  0.10 mm {0.0039 in}

3. Measure the contact surface of the exhaust manifold and the intake manifold as shown in the figure for distortion using a straight edge and feeler gauge.

bezeze00000030

  • If it exceeds the maximum specification, grind the surface or replace the cylinder head.

  Maximum distortion

  0.05 mm {0.002 in}

  Maximum grinding

  0.20 mm {0.008 in}