#
CLUTCH MASTER CYLINDER REMOVAL/INSTALLATION

id051000801400

  Caution

  • Be careful not to spill clutch fluid on a painted surface. If this should happen, wash it off immediately.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. Bleed the air. (See CLUTCH FLUID REPLACEMENT.)

4. Inspect the clutch pedal. (See CLUTCH PEDAL INSPECTION.)

1 | Hose clamp
2 | Reserve hose
3 | Clutch pipe
4 | Clutch return spring (See Clutch Return Spring, E-Clip Removal Note.) (See Clutch Return Spring, E-Clip Installation Note.)
5 | E-Clip (See Clutch Return Spring, E-Clip Removal Note.) (See Clutch Return Spring, E-Clip Installation Note.)
6 | Bracket
7 | Clutch master cylinder (See Clutch Master Cylinder Installation Note.)
8 | Pedal assembly
9 | Stopper rubber
10 | Stopper

## Clutch Return Spring, E-Clip Removal Note

1. Loosen the clutch master cylinder and bracket installation bolt.

## Clutch Master Cylinder Installation Note

1. Hold the joint as shown.

## Clutch Return Spring, E-Clip Installation Note

1. Lightly tighten the clutch master cylinder and bracket installation bolt.