#
BEFORE REPAIR PROCEDURE

id011400802000

  Warning

  • Fuel vapor is hazardous. It can very easily ignite, causing serious injury and damage. Always keep sparks and flames away from fuel.
  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, always complete the "Fuel Line Safety Procedure".
  • A person charged with static electricity could cause a fire or explosion, resulting in death or serious injury. Before performing work on the fuel system, discharge static electricity by touching the vehicle body.

  Caution

  • If there is foreign material on the connecting area of the quick release connector, it might damage the connector or fuel pipe. To prevent this, disconnect the connector and clean the connecting area before connecting.

## Fuel Line Safety Procedure

1. Remove the fuel-filler cap to release the pressure inside the fuel tank.

2. Remove the fuel pump relay.

3. Start the engine.

4. After engine stalling, crank the engine 2-3 times.

5. Turn the ignition switch to the LOCK position.

6. Install the fuel pump relay.