#
PANEL LIGHT CONTROL SWITCH INSPECTION

id091800806400

1. Connect the connector to the panel light control switch.

2. Connect the negative battery cable.

3. Measure the voltage at the panel light control switch using a voltmeter.

  • When inspecting terminal B for continuity, disconnect the panel light control switch connector.

4. If the value are not as specified in the Terminal Voltage List (Reference), inspect the parts under "Inspection item (s)" and related wiring harnesses.

5. If the system does not work properly even though the parts or related wiring harnesses do not have any malfunction, replace the panel light control switch.

## Terminal Voltage Table (Reference)

Terminal | Signal | Connected to | Test condition | Voltage (V)/Continuity | Inspection item (s)
--- | --- | --- | --- | --- | ---
D | Illumination | Each illumination | Inspect using an oscilloscope. (See Terminal D inspection) | - | • Each illumination • Related harness
F | TNS | TNS relay | Headlight switch is at TNS or headlight position. | B+ | • TNS relay (See RELAY INSPECTION) • ILLUMI 10A fuse • Related harness
Other | 0
H | Ground | GND | Under any condition: Inspect for continuity to ground. | Yes | • GND • Related harness

### Terminal D inspection

1. Measure the wave pattern of the terminal D on the panel light control switch using an oscilloscope.

2. Set the headlight switch to either the TNS or headlight position.

3. Set the panel light control switch to the brightest position.

4. Verify that the pattern on the screen is as shown in the figure.

5. Verify that the pattern on the screen matches the pattern shown in the figure as the panel light control switch is gradually turned to the darkest position.