#
INSTRUMENT CLUSTER STRUCTURAL VIEW

id092200101200

X: Applied

No. | Warning and indicator lights | Input signal source | CAN system | Note
--- | --- | --- | --- | ---
1 | Security light | PCM | - | -
2 | Seat belt warning light | Buckle switch | - | -
3 | Oil pressure warning light | Oil pressure switch | - | -
4 | Brake system warning light | • Parking brake switch • Brake fluid level sensor | - | -
ABS HU/CM | X | Vehicles with ABS
5 | Door ajar warning light | Door switch | - | -
6 | Air bag system warning light | SAS unit | - | -
7 | Generator warning light | PCM | X | -
8 | MIL | PCM | X | -
9 | Turn indicator light | Turn switch | - | -
10 | High-beam indicator light | Headlight switch | - | -
11 | ABS warning light | ABS HU/CM | X | Vehicles with ABS
12 | HOLD indicator light | PCM | X | ATX
13 | Selector indicator light | PCM | X | ATX
14 | Fuel-level warning light | Fuel gauge sender unit | - | -