#
DOOR SPEAKER REMOVAL/INSTALLATION

id092000807200

1. Disconnect the negative battery cable.

2. Remove the door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.) (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Door speaker (See Door Speaker Installation Note)

4. Install in the reverse order of removal.

## Door Speaker Installation Note

1. Attach the speaker with the wiring harness placed in the groove of the door unit panel.

  Caution

  • If the door speaker is installed with the wiring harness out of the groove, the following malfunctions could occur. Therefore, when installing the door speaker, always be sure the wiring harness is in the groove.

  - Open circuit in the wiring harness
  - Water penetration into the door trim
  - Abnormal noise due to a vibrating wiring harness