#
GENERATOR REMOVAL/INSTALLATION [ZJ, ZY]

id011700800224

  Warning

  • When the battery cables are connected, touching the vehicle body with generator terminal B generates sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the negative battery cable before performing the following operation.

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the front combination light. (RH) (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Position the P/S oil pump out of the way with the pipes still connected.

5. Remove the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, ZY].)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

P/S oil pump pipe tightening torque

  7.8-10.8 N·m {80-110 kgf·cm, 70-95 in·lbf}

1 | Terminal B cable
2 | Generator connector
3 | Generator (See Generator Removal Note.)

## Generator Removal Note

1. Remove bolt A with the generator since there is not enough space.