#
DTC P0480

id010200807400

DTC P0480 | Cooling fan relay No.1 control circuit malfunction
--- | ---
DETECTION CONDITION | • The PCM monitors the cooling fan relay No.1 control signal at PCM terminal 1AT. If the PCM detects that the cooling fan relay No.1 control signal does not change the coolant temperature to 100 °C {212 °F} or more, the PCM determines that the cooling fan relay No.1 control has a malfunction. Diagnostic support note • This is continuous monitor (other) • The MIL does not illuminate. • The PENDING CODE is available if the PCM detects above malfunction condition during the first drive cycle. • The FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Cooling fan relay No.1 malfunction • Connector or terminal malfunction • Open circuit in wiring between the ENGINE fuse and cooling fan relay No.1 terminal E • Open circuit in wiring between cooling fan relay No.1 terminal A and PCM terminal 1AT • Short to ground in wiring between cooling fan relay No.1 terminal A and PCM terminal 1AT • Short to power circuit between cooling fan relay No.1 terminal A and PCM terminal 1AT • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | PERFORM DTC CONFIRMATION PROCEDURE • Perform the DTC CONFIRMATION PROCEDURE. (See DTC CONFIRMATION PROCEDURE.) • Is the same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Go to the INTERMITTENT CONCERN TROUBLESHOOTING procedure. (See INTERMITTENT CONCERN TROUBLESHOOTING.)
2 | INSPECT COOLING FAN RELAY NO.1 CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the cooling fan relay No.1 connector. • Inspect for poor connection (such as damaged, pulled-out pins, and corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal and/or connector, then go to Step 9.
No | Go to the next step.
3 | INSPECT COOLING FAN RELAY NO.1 POWER FOR OPEN CIRCUIT • Turn the ignition switch to the ON position. (Engine off). • Measure the voltage between cooling fan relay No.1 terminal E (wiring harness-side) and body ground. • Is the voltage B+? | Yes | Go to the next step.
No | Replace or replace the wiring harness for an open circuit, then go to Step 9.
4 | INSPECT COOLING FAN RELAY NO.1 • Inspect cooling fan relay No.1. (See RELAY INSPECTION.) • Is cooling fan relay No.1 normal? | Yes | Go to the next step.
No | Replace the cooling fan relay No.1, then go to Step 9.
5 | INSPECT COOLING FAN RELAY NO.1 CONTROL CIRCUIT FOR SHORT TO POWER • Measure the voltage between cooling fan relay No.1 terminal A (wiring harness-side) and body ground. • Is voltage B+? | Yes | Repair or replace the wiring harness for short to power, then go to Step 9.
No | Go to the next step.
6 | INSPECT COOLING FAN RELAY NO.1 CONTROL CIRCUIT FOR SHORT TO GROUND • Inspect for continuity between cooling fan relay No.1 terminal A (wiring harness-side) and body ground. • Is there continuity? | Yes | Repair or replace the wiring harness for an open circuit, then go to Step 9.
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged, pulled-out pins, and corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal and/or connector, then go to Step 9.
No | Go to the next step.
8 | INSPECT COOLING FAN RELAY NO.1 CONTROL CIRCUIT FOR OPEN CIRCUIT • Inspect for continuity between cooling fan relay No.1 terminal A (wiring harness-side) and PCM terminal 1AT (wiring harness-side). • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for an open circuit, then go to the next step.
9 | VERIFY TROUBLESHOOTING OF DTC P0480 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Perform the KOEO/KOER self-test. (See KOEO/KOER SELF-TEST.) • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION.)
No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE.) • Are any DTCs present? | Yes | Go to applicable DTC troubleshooting. (See DTC TABLE.)
No | Troubleshooting completed.