#
SCHEDULED MAINTENANCE TABLE

id000000801200

## For Australia and New Zealand

Chart symbols:

  I :
Inspect: Inspect and clean, repair, adjust, or replace if necessary.
  R :
Replace
  T :
Tighten
  C :
Clean

Remarks:

• To ensure efficient operation of the engine and all systems related to emission control, the ignition and fuel systems must be serviced regularly. It is strongly recommended that all servicing related to these systems be completed by an authorized Mazda Dealer. • After the prescribed period, continue to follow the described maintenance at the recommended intervals. • Refer to the following for a description of items marked* in the maintenance chart.
*1: | Also inspect and adjust the power steering and air conditioner drive belts, if installed.
*2: | If the vehicle is operated under any of the following conditions, change the engine oil and oil filter more often than recommended intervals.
| a. Driving in dusty conditions. b. Extended periods of idling or low speed operation. c. Driving for long period in cold temperatures or driving regularly at short distance only.
*3: | If the vehicle is operated in very dusty or sandy areas, inspect and if necessary, clean or replace the air cleaner element more often than the recommended intervals.
*4: | This is a full function check of electrical systems such as lights, wiper and washer systems (including wiper blades), and power windows.
*5: | If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, change the brake fluid annually.

Maintenance Item | Maintenance Interval (Number of months or km (miles), whichever comes first)
--- | ---
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60 | 66 | 72 | 78 | 84 | 90 | 96
×1000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | 120 | 130 | 140 | 150 | 160
×1000 miles | 6.25 | 12.5 | 18.75 | 25 | 31.25 | 37.5 | 43.75 | 50 | 56.25 | 62.5 | 68.75 | 75 | 81.25 | 87.5 | 93.75 | 100
ENGINE
Drive belts | *1 | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Engine oil | *2 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Oil filter | *2 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
COOLING SYSTEM
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | Replace at first 80,000 km (50,000 miles) or 48 months; after that, every 24 months
FUEL SYSTEM
Idle speed |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Air cleaner element | *3 |  | C |  | C |  | R |  | C |  | C |  | R |  | C |  | C
Fuel filter |  |  |  | R |  |  |  | R |  |  |  | R |  |  |  | R
Fuel lines & hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
IGNITION SYSTEM
Spark plugs |  |  |  | R |  |  |  | R |  |  |  | R |  |  |  | R
EMISSION CONTROL SYSTEM
Evaporative system (if installed) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
ELECTRICAL SYSTEM
Battery electrolyte level & specific gravity |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
All electrical system | *4 |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
CHASSIS & BODY
Brake and clutch pedals | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Brake lines, hoses & connections |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake fluid | *5 | I | I | I | R | I | I | I | R | I | I | I | R | I | I | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit & hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Drum brakes |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Power steering fluid, lines, hoses, and connections | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation & linkages |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Manual transaxle oil |  |  |  |  |  |  |  |  |  | R |  |  |  |  |  |
Automatic transmission fluid level |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Front & rear suspension & ball joints |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Drive shaft dust boots |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Bolts & nuts on chassis & body |  | T |  | T |  | T |  | T |  | T |  | T |  | T |  | T
Exhaust system heat shields |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I

## Except for Australia and New Zealand

Chart symbols:

  I :
Inspect: Inspect and clean, repair, adjust, or replace if necessary.
  R :
Replace
  T :
Tighten
  C :
Clean

Remarks:

• To ensure efficient operation of the engine and all systems related to emission control, the ignition and fuel systems must be serviced regularly. It is strongly recommended that all servicing related to these systems be completed by an authorized Mazda Dealer. • After the prescribed period, continue to follow the described maintenance at the recommended intervals. • Refer to the following for a description of items marked* in the maintenance chart.
*1: | Also inspect and adjust the power steering and air conditioner drive belts, if installed.
*2: | If the vehicle is operated under any of the following conditions, change the engine oil and oil filter more often than recommended intervals.
| a. Driving in dusty conditions. b. Extended periods of idling or low speed operation. c. Driving for long period in cold temperatures or driving regularly at short distance only.
*3: | If the vehicle is operated in very dusty or sandy areas, inspect and if necessary, clean or replace the air cleaner element more often than the recommended intervals.
*4: | This is a full function check of electrical systems such as lights, wiper and washer systems (including wiper blades), and power windows.
*5: | If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, change the brake fluid annually.

Maintenance Item | Maintenance Interval (Number of months or km (miles), whichever comes first)
--- | ---
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60 | 66 | 72 | 78 | 84 | 90 | 96
×1000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | 120 | 130 | 140 | 150 | 160
×1000 miles | 6.25 | 12.5 | 18.75 | 25 | 31.25 | 37.5 | 43.75 | 50 | 56.25 | 62.5 | 68.75 | 75 | 81.25 | 87.5 | 93.75 | 100
ENGINE
Drive belts | *1 | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Engine oil | *2 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Oil filter | *2 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
COOLING SYSTEM
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | Replace every 2 years
FUEL SYSTEM
Idle speed |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Air cleaner element | *3 |  | C |  | C |  | R |  | C |  | C |  | R |  | C |  | C
Fuel filter |  |  |  | R |  |  |  | R |  |  |  | R |  |  |  | R
Fuel lines & hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
IGNITION SYSTEM
Spark plugs |  |  |  | R |  |  |  | R |  |  |  | R |  |  |  | R
EMISSION CONTROL SYSTEM
Evaporative system (if installed) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
ELECTRICAL SYSTEM
Battery electrolyte level & specific gravity |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
All electrical system | *4 |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
CHASSIS & BODY
Brake and clutch pedals | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Brake lines, hoses & connections |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake fluid | *5 | I | I | I | R | I | I | I | R | I | I | I | R | I | I | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit & hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Drum brakes |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Power steering fluid, lines, hoses, and connections | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation & linkages |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Manual transaxle oil |  |  |  |  |  |  |  |  |  | R |  |  |  |  |  |
Automatic transmission fluid level |  | I |  | I |  | I |  | I |  |  |  | I |  | I |  | I
Automatic transmission fluid |  |  |  |  | R |  |  |  |  | R |  |  |  |  | R |
Front & rear suspension & ball joints |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Drive shaft dust boots |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Bolts & nuts on chassis & body |  | T |  | T |  | T |  | T |  | T |  | T |  | T |  | T
Exhaust system heat shields |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Body condition (for rust, corrosion & perforation) | Inspect annually