#
CYLINDER HEAD (II) ASSEMBLY

id011000504400

1. Assemble in the order indicated in the table.

1 | Cylinder head gasket
2 | Cylinder head (See Cylinder Head Assembly Note)
3 | Tappet
4 | Camshaft (See Camshaft Assembly Note)
5 | Camshaft cap (See Camshaft Assembly Note)
6 | Camshaft sprocket, variable valve timing actuator (See Camshaft Sprocket, Variable Valve Timing Actuator Assembly Note)
7 | Water outlet

## Cylinder Head Assembly Note

1. Tighten the cylinder head installation bolts in three steps in the order shown in the figure.

  (1)Tightening torque
  17.5-22.5 N·m {1.79-2.29 kgf·m, 13.0-16.5 ft·lbf}
  (2)Tightening angle
  85°-95°
  (3) Tightening angle
  85°-95°

## Camshaft Assembly Note

  Note

  • Install the camshaft with the No.1 camshaft positioned at TDC of the compression stroke.

1. Install the camshaft cap to the position shown in the figure, and temporarily tighten the No.2 and No.7 camshaft installation bolts.

2. Tighten the camshaft cap installation bolts in two to three passes uniformly in the order shown in the figure.

  Tightening torque
  11.3-14.2 N·m {1.16-1.44 kgf·m, 8.4-10.4 ft·lbf}

## Camshaft Sprocket, Variable Valve Timing Actuator Assembly Note

1. Fix the camshaft using a suitable wrench on the cast hexagon as shown in the figure.

2. Tighten the camshaft sprockets and variable valve timing actuator installation bolts.

  Tightening torque
  49.6-60.8 N·m {5.06-6.19 kgf·m, 36.6-44.8 ft·lbf}