#
WATER PUMP REMOVAL/INSTALLATION [ZJ, ZY]

id011200800719

1. Disconnect the negative battery cable.

2. Remove the splash shield.

3. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT [ZJ, ZY].)

4. Remove the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, ZY].)

5. Remove the crankshaft pulley. (See TIMING CHAIN REMOVAL/INSTALLATION [ZJ, ZY].)

6. Position the generator out of the way. (See GENERATOR REMOVAL/INSTALLATION [ZJ, ZY].)

7. Remove in the order indicated in the table.

1 | Water pump component
2 | O-ring

8. Install in the reverse order of removal.

9. Add the engine coolant. (See ENGINE COOLANT REPLACEMENT [ZJ, ZY].)

10. Inspect the system for engine coolant leakage. (See ENGINE COOLANT LEAKAGE INSPECTION [ZJ, ZY].)