#
POWER STEERING OIL PUMP REMOVAL/INSTALLATION

id061400800700

1. Remove the air cleaner. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITHOUT WU-TWC].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].)

2. Remove the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, ZY].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Pressure switch connector
2 | Pressure pipe
3 | Return hose
4 | Power steering oil pump