#
NO.28 HOLD INDICATOR LIGHT ILLUMINATES WHEN HOLD SWITCH IS NOT TURNED TO ON [FN4A-EL]

id0503a1815500

28 | HOLD indicator light illuminates when HOLD switch is not turned to ON
DESCRIPTION | • HOLD indicator light in dashboard illuminates even though HOLD switch is turned off and IG SW at ON.
POSSIBLE CAUSE | • HOLD switch or related wiring harness malfunction.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Check the HOLD switch (See HOLD SWITCH INSPECTION [FN4A-EL].) • Is HOLD switch normal? | Yes | Go to next step.
No | Repair or replace any defective parts.
2 | • Disconnect PCM. • Turn ignition switch off. • Is resistance between 3Q terminal at the PCM connector and body ground more than 10 kilohms? | Yes | Replace PCM.
No | Inspect following wiring harnesses • Between instrument cluster terminal 2W and PCM terminal 1S • Between instrument cluster terminal 2X and PCM terminal 1W
3 | • Verify test results. - If normal, return to diagnostic index to service any additional symptoms. - If malfunction remains, inspect related Service Information and perform repair or diagnosis. • If vehicle repaired, troubleshooting completed. • If vehicle not repaired or additional diagnostic information not available, replace PCM.