#
BOLT INSPECTION

id011000503300

1. Measure the length of each bolt.

  • If it exceeds the maximum specification, replace the bolt.

  Standard cylinder head bolt length• •
  128.9-129.5 mm {5.075 -5.098 in}
  Maximum cylinder head bolt length
  130.2 mm {5.125 in}
  Standard connecting rod bolt length
  ZJ: 36.2-36.6 mm {1.426 -1.440 in}
  ZY, Z6: 46.7-47.3 mm {1.839 -1.862 in}
  Maximum connecting rod bolt length
  ZJ: 36.95 mm {1.454 in}
  ZY, Z6: 48.0 mm {1.889 in}