#
NO.27 HOLD INDICATOR LIGHT DOES NOT ILLUMINATE WHEN HOLD SWITCH IS TURNED TO ON [FN4A-EL]

id0503a1815400

27 | HOLD indicator light does not illuminate when HOLD switch is turned to ON
DESCRIPTION | • HOLD indicator light in dashboard does not illuminate when HOLD switch is turned on and IG SW at ON.
POSSIBLE CAUSE | • HOLD switch, HOLD indicator light or related wiring harness malfunction.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Are other indicator lights illuminated with ignition switch is at ON? | Yes | Inspect meter fuse.
No | Go to next step.
2 | • Check the HOLD switch (See HOLD SWITCH INSPECTION [FN4A-EL].) • Is HOLD switch normal? | Yes | Go to next step.
No | Repair or replace any defective parts.
3 | • Disconnect PCM. • Turn ignition switch on. • Is voltage between 3Q terminal at the PCM connector and body ground more than 10.5 V? | Yes | Replace PCM.
No | Reconnect PCM. Go to next step.
4 | • Inspect instrument cluster operation. (See INSTRUMENT CLUSTER INSPECTION.) • Is any malfunction detected? | Yes | Repair or replace malfunctioning part according to inspection result.
No | Inspect following wiring harnesses • Between instrument cluster terminal 2W and PCM terminal 1S • Between instrument cluster terminal 2X and PCM terminal 1W
5 | • Verify test results. - If normal, return to diagnostic index to service any additional symptoms. - If malfunction remains, inspect related Service Information and perform repair or diagnosis. • If vehicle repaired, troubleshooting completed. • If vehicle not repaired or additional diagnostic information not available, replace PCM.