#
STARTER INSPECTION [ZJ, ZY]

id011900800315

## On-vehicle Inspection

1. Verify that the battery is fully charged.

2. Verify that the starter rotates smoothly without any noise when the engine is cranked.

  • If the starter does not operate normally, inspect the following.

  - Remove the starter, and inspect the starter.
  - Inspect the related wiring harness, the ignition switch, and the transaxle range switch (ATX).

## No Load Test

1. Verify that the battery is fully charged.

2. Connect the starter, battery, and a tester as shown in the figure.

3. Operate the starter and verify that it rotates smoothly.

  • If the starter does not operate smoothly, inspect the starter.

4. Measure the voltage and current while the starter is operating.

  • If it is less than the specification, replace the starter.

Starter no load test voltage

  11 V

Starter no load test current

  90 A or less