#
SIDE PROTECTOR INSTALLATION

id091600801200

1. Remove the adhesive remaining on the side protector and the body using a razor.

  Warning

  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

2. Remove any grease or dirt from the adhesion surface of the side protector and the body.

3. Attach double-sided adhesive tape to the side protector as shown in the figure.

Attachment areas

  a: 29-31 mm {1.15-1.22 in}
  b: 2.0-4.0 mm {0.08-0.15 in}
  c: 11-13 mm {0.44-0.51 in}
  d: 2.0-4.0 mm {0.08-0.15 in}
  e: 1.0-3.0 mm {0.04-0.11 in}
  f: 5.0 mm {0.2 in}
  g: 1.0-3.0 mm {0.04-0.11 in}

4. Peel off the backing paper from the double-sided adhesive tape and attach the side protector onto the body as shown in the figure.

Clearance

  a: 1.2-4.2 mm {0.05-0.16 in}
  b: 3.6-6.6 mm {0.14-0.25 in}