#
SUSPENSION SPECIFICATIONS

id020000100300

Item | Specification
--- | ---
Front suspension | Type | Strut
Spring type | Coil spring
Shock absorber type | Cylindrical, double-acting (Low-pressure gas charged)
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | 18.5 {0.73}
Wheel alignment (Unloaded)*1 | Total toe-in | Tire [Tolerance ±4 {0.16}] | (mm {in}) | 3 {0.12}
Rim inner | 14 inch wheel: 1.8±2.4 {0.07±0.09} 15 inch wheel: 2.0±2.6 {0.08±0.10}
(degree) | 0°19'±0°24'
Maximum steering angle [Tolerance ±3°] | inner | 39°
outer | 32°
Caster angle*2 [Tolerance ±1°] | 3°34' (reference value)
Camber angle*2 [Tolerance ±1°] | -0°31' (reference value)
Steering axis inclination | 12°59' (reference value)
Rear suspension | Type | Torsion beam axle
Spring type | Coil spring
Shock absorber type | Cylindrical, double-acting (Hi-pressure gas charged)
Wheel alignment (Unloaded)*1 | Total toe-in | Tire [Tolerance ±4 {0.16}] | (mm {in}) | 5 {0.2} (reference value)
Rim inner | 14 inch wheel: 3.0±2.4 {0.12±0.09} (reference value) 15 inch wheel: 3.3±2.6 {0.13±0.10} (reference value)
(degree) | 0°28'±0°24' (reference value)
Camber angle*2 [Tolerance ±1°] | -1°02' (reference value)
Thrust angle [Tolerance ±0°48'] | (degree) | 0° (reference value)

  *1 :
Engine coolant and engine oil are at specified level. Fuel is full. Spare tire, jack and tools are in designated position.
  *2 :
Difference between left and right must not exceed 1°30'.