#
MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR [WITH WU-TWC]

id0140001639d2

## Function

• Detects the intake air pressure inside the intake manifold in order to monitor EGR system operation.

## Structure

• Installed on the intake manifold.

## Operation

• A piezoelectric element is enclosed in the sensor and the electric potential difference changes as the MAP decreases. The output voltage decreases as the MAP decreases.