#
VALVE, VALVE GUIDE INSPECTION

id011000506200

1. Measure the valve head margin thickness using a vernier caliper.

  • If not within the specification, replace the valve.

  Standard valve head margin thickness
  1.6-2.0 mm {0.063-0.078 in}

2. Measure the length of each valve using the vernier caliper.

  • If it is less than the minimum specification, replace the valve.

Standard valve length (mm {in})

Valve | ZJ | ZY, Z6
--- | --- | ---
IN | 98.01-98.61 {3.859-3.882} | 96.80-97.40 {3.812-3.834}
EX | 98.44-99.04 {3.876-3.899} | 96.30-96.90 {3.792-3.814}

Minimum valve length (mm {in})

Valve | ZJ | ZY, Z6
--- | --- | ---
IN | 97.79 {3.850} | 96.58 {3.802}
EX | 98.22 {3.867} | 96.08 {3.783}

3. Measure the stem diameter of each valve using the micrometer. Measurement positions total six and they are in the X and Y directions at the three points (A, B, and C) as shown in the figure.

  • If it is less than the minimum specification, replace the valve.

  Standard valve stem diameter
  IN: 5.470-5.485 mm {0.2154-0.2159 in}
  EX: 5.465-5.480 mm {0.2152-0.2157 in}
  Minimum valve stem diameter
  IN: 5.424 mm {0.2136 in}
  EX: 5.419 mm {0.2134 in}

4. Measure the inner diameter of each valve guide using the caliper gauge. Measurement positions total six and they are in the X and Y directions at the three points (A, B, and C) as shown in the figure.

  • If not within the specification, replace the valve guide.

  Standard valve guide inner diameter
  5.510-5.530 mm {0.2170-0.2177 in}

5. Calculate the clearance between the valve stem and the valve guide by subtracting the inner diameter of the valve guide from the outer diameter of the corresponding valve stem.

  • If it exceeds the maximum specification, replace the valve or the valve guide, or both.

  Standard clearance
  IN: 0.025-0.060 mm {0.0010-0.0023 in}
  EX: 0.030-0.065 mm {0.0012-0.0025 in}
  Maximum clearance
  0.10 mm {0.04 in}

6. Measure the protrusion height (dimension A) of each valve guide using the vernier caliper.

  • If not within the specification, replace the valve guide

  Standard height
  12.2-12.8 mm {0.49-0.50 in}