#
HORN REMOVAL/INSTALLATION

id092200800900

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the washer tank installation bolt and move the washer tank rearward. (See WASHER TANK REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Bolt
2 | Connector
3 | Horn

5. Install in the reverse order of removal.