#
ON-BOARD DIAGNOSTIC ACTIVE COMMAND MODES FUNCTION

id040200175300
• This function allows control of devices through the WDS or equivalent.

Active Command Modes Table

Command Name | Definition | Operation | Note
--- | --- | --- | ---
PMP_MOTOR | ABS motor | On/Off | Ignition key at ON (Engine running, vehicle is not moving)
LR_OUTLET | Left rear ABS pressure reduction solenoid valve | On/Off
LR_INLET | Left rear ABS pressure retention solenoid valve | On/Off
RR_INLET | Right rear ABS pressure retention solenoid valve | On/Off
RR_OUTLET | Right rear ABS pressure reduction solenoid valve | On/Off
LF_INLET | Left front ABS pressure retention solenoid valve | On/Off
LF_OUTLET | Left front ABS pressure reduction solenoid valve | On/Off
RF_INLET | Right front ABS pressure retention solenoid valve | On/Off
RF_OUTLET | Right front ABS pressure reduction solenoid valve | On/Off