#
B-PILLAR LOWER TRIM REMOVAL/INSTALLATION

id091700458900

1. Remove the front scuff plate. (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

2. Remove the rear scuff plate. (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

3. Extend the upper B-pillar lower trim and remove the tab.

4. Pull the B-pillar lower trim, then remove clips A and pin B from the body.

5. Remove the B-pillar lower trim.

6. Install in the reverse order of removal.