#
REAR WIPER MOTOR REMOVAL/INSTALLATION

id091900475500

1. Disconnect the negative battery cable.

2. Remove the liftgate trim. (See LIFTGATE TRIM REMOVAL/INSTALLATION.)

3. Remove the rear wiper arm and blade. (See REAR WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Rear wiper motor
4 | Outer bushing

5. Install in the reverse order of removal.

6. Adjust the rear wiper arm and blade. (See REAR WIPER ARM AND BLADE ADJUSTMENT.)