#
PRECAUTION (SUSPENSION)

id021000800100

## Wheel And Tire Removal/Installation

1. When installing a wheel, tighten the wheel nuts in opposing diagonal order to the following torque.

Tightening torque

  88.2-117.6 N·m {9.00-11.99 kgf·m, 65.06-86.73 ft·lbf}

## Suspension Links Removal/Installation

  Note

  • To prevent the bushings from being twisted or pinched, perform the procedures with no passengers or luggage aboard the vehicle.

1. For the joint section with rubber bushings, raise the vehicle using a lift, and then temporarily tighten the installation bolts and nuts. After the vehicle has been lowered to the ground, tighten them to the specified torque.

## Brake Lines Disconnection/Connection

1. If any brake line has been disconnected anytime during the procedures, add brake fluid, bleed the brakes, and inspect for leakage after the procedure has been completed.