POSITIVE CRANKCASE VENTILATION (PCV) VALVE INSPECTION

id011600800400

1. Remove the intake manifold. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITHOUT WU-TWC], INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].)

2. Remove the PCV valve and the oil separator as a single unit.

3. Verify that there is no airflow when pressure is applied to port A.

am2uuw00000041

  • If there is airflow, replace the PCV valve and the oil separator as a single unit.

  Oil separator tightening torque

  8—10 N·m {82—101 kgf·cm, 71—88 in·lbf}

4. Verify that there is airflow when vacuum is applied to port A.

  • If there is no airflow, replace the PCV valve and the oil separator as a single unit.