#
VEHICLE SPEEDOMETER SENSOR REMOVAL/INSTALLATION (WITHOUT ABS) [F35M-R]

id0515008429a5

1. Disconnect the negative battery cable.

2. Remove the battery and battery tray.

3. Separate the cable bracket.

4. Disconnect the vehicle speedometer sensor connector.

5. Remove the vehicle speedometer sensor.

6. Apply transmission oil to a new O-ring and install it on a vehicle speedometer sensor.

7. Install the vehicle speedometer sensor.

Tightening torque

  7.8-11 N·m {80-112 kgf·cm, 70-97 in·lbf}

8. Connect the vehicle speedometer sensor connector.

9. Install the cable bracket.

10. Install the battery and battery tray.

11. Connect the negative battery cable.