#
PID/DATA MONITOR AND RECORD [WITHOUT WU-TWC]

id0102001005d7
• The PID/DATA monitoring items are as shown in the table below.

Monitor item table

-: Not applicable

PID item | Definition | Unit/Condition | PCM terminal
--- | --- | --- | ---
A/CL V | Refrigerant pressure switch (middle) | V | 1U
A/CT | Evaporator temperature | °C, °F | 1AD
A/CT V | Evaporator temperature (voltage) | V | 1AD
ACCS | A/C relay | On/Off | 1AL
ACSW | A/C switch | On/Off | 1Q
ALTF | Generator field coil control duty value | % | 2AN
ALTT V | Generator output voltage | V | 2AR
ARPMDES | Target engine speed | RPM | -
BOO | Brake switch | On/Off | 1V
CPP*1 | Clutch pedal position | On/Off | 1P
CPP/PNP*1 | Shift lever position | Drive/Neutral | 1AB
DTCCNT | Number of DTC detected | - | -
ECT | Engine coolant temperature | °C, °F | 2J
Engine coolant temperature (voltage) | V | 2J
EVAPCP | Purge solenoid valve duty value | % | 2AV
FAN1 | Fan relay No.1 control | On/Off | 1AT
FAN2 | Fan relay No.2 control | On/Off | 1I
FP | Fuel pump relay | On/Off | *41AC
*51AH
FUELPW | Fuel injector duration | ms | 2B, 2C, 2D, 2H
FUELSYS | Fuel system status | OL_Drive/ OL/ CL_Fault/ OL_Fault/ CL | -
GENVDSD | Generator voltage desired | V | -
HTR11 | HO2S heater control | On/Off | 2AM
IAC | IAC valve control | % | 2X, 2AB
IAT | Intake air temperature | V | 2AQ
Intake air temperature (voltage) | °C, °F | 2AQ
IMRC | VTCS | On/Off | 2AF, 2AJ
IMTV*3 | VIS | On/Off | 2AO, 2AS
INGEAR | Gears are engaged. | On/Off | *11P, 1AB
*2-
IVS | CTP condition | Idle/Off Idle | 2AA
KNOCKR | Knocking retard | ° | 2BA
LOAD | Engine load (charging efficiency) | % | -
LONGFT1 | Long term fuel trim | % | -
MAF | Mass air flow | g/s | 2AU
Mass air flow (voltage) | V | 2AU
MIL | Malfunction indicator lamp | On/Off | -
MIL_DIS | Travelled distance since MIL illuminated | km, mile | -
O2S11 | HO2S | V | 2AI
Rich/Lean
PSP | PSP switch | High/Low | 2AC
RFCFLAG | Readiness function code | Learnt/Not Learnt | -
RPM | Engine speed | RPM | 2P
SHRTFT1 | Short term fuel trim | % | -
SPARKADV | Ignition timing | ° (BTDC) | 2BB
test | Test mode | On/Off | -
TP | TP | % | 2AA
TP (voltage) | V | 2AA
TP REL | Throttle position signal (relative value) | % | 2AA
TPCT | TP sensor voltage at CTP | V | 2AA
VPWR | Battery positive voltage | V | 1AX, 1BF, 1BG
VSS | Vehicle speed | KPH, MPH | *11AA, 1AE
*21AY, 1BC
VT DUTY1 | OCV control | % | 2AK, 2AG

  *1 :
MTX
  *2 :
ATX
  *3 :
ZY
  *4 :
With immobilizer system
  *5 :
Without immobilizer system