#
FRONT COMBINATION LIGHT REMOVAL/INSTALLATION

id091800464400

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Bracket
4 | Fastener
5 | Front combination light

4. Install in the reverse order of removal.

5. Adjust the headlight aiming. (See HEADLIGHT AIMING.)