#
COOLING FAN MOTOR INSPECTION [ZJ, ZY]

id011200801819

1. Verify that the battery is fully charged.

2. Connect the battery positive voltage and a tester to the fan motor connector as shown in the figure.

Item | Polarity | Terminal
--- | --- | ---
High | + | c and d
- | a and b
Low | + | c or d
- | a and b

3. Verify that the fan motor operates smoothly at the standard current draw.

  • If the fan motor does not operate normally, replace it.

Cooling fan motor current

  High: 7.9-13.9 A
  Low: 5.8-11.8 A