#
PANEL LIGHT CONTROL SWITCH REMOVAL/INSTALLATION

id091800806500

1. Disconnect the negative battery cable.

2. Remove the side panel. (See SIDE PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Panel light control switch (See Panel Light Control Switch Removal Note)
2 | Connector

4. Install in the reverse order of removal.

## Panel Light Control Switch Removal Note

1. Insert your hand into the dashboard from where the driver-side side panel was removed, and squeeze the tabs of the panel light control switch.

2. Pull the panel light control switch outward to remove it.