VALVE CLEARANCE ADJUSTMENT [ZJ, ZY]

id0110005036b7

1. Disconnect the negative battery cable.

2. Remove the front tire (RH).

3. Remove the ignition coil. (See IGNITION COIL REMOVAL/INSTALLATION [ZJ, ZY].)

4. Remove the ventilation hose.

5. Remove the cylinder head cover.

6. Remove the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, ZY].)

7. Remove the engine front cover blind plug as shown in the figure.

am2zzw00004422

8. Insert a M10 or M6 bolt (45—80 mm {1.8—3.1 in} length bolt with threads to the end) into the service hole (right side) by hand as shown in the figure. Pull back the inserted bolt approx. 2 mm {0.08 in} from where it contacts the tensioner arm (loosen the M10 bolt approx. two turns), and set the bolt in a position slightly outward of the tensioner arm.

Insert Bolt | Front Cover Service Hole
--- | ---
M10 × 1.25 | 10 mm {0.39 in}
M6 × 1.25 | 7 mm {0..3 in}

am2zzw00004249

9. Release tension on the timing chain.

  (1) Press down the link plate of the chain tensioner from the service hole on the left side using a thin flathead screwdriver (precision screwdriver) as shown in the figure. Then rotate the crank pulley backwards (counterclockwise) with the plunger lock released.

  am2zzw00004250

    Note
    • When the crankshaft pulley is turned counterclockwise, the timing chain loosens because the tensioner arm is pressed by the timing chain and the plunger of the chain tensioner is pressed in.

    am2zzw00004251

  (2) Insert the M10 or M6 bolt installed to the engine front cover to the position where it catches the inside of the rib on the tensioner arm.

  am2zzw00004252

    Note
    • When the timing chain loosens, the tensioner arm moves to the position shown in the figure and presses the M10 or M6 bolt to secure the tensioner arm.

    am2zzw00004253

10. Fix the camshaft using a wrench on the cast hexagon. Remove the camshaft sprocket installation bolt.

am2zzw00004254

11. Remove the timing sprocket on the exhaust side with the timing chain positioned out of the way.

am2zzw00004255

12. Loosen the camshaft cap installation bolts in two or three steps in the order shown in the figure, and remove the camshaft caps.

am2zzw00004256

13. Remove the intake and exhaust camshafts.

14. Remove the tappet.

15. Select a proper tappet according to the result of the valve clearance inspection and install it.

Tappet to be selected: thickness of the removed tappet + measured valve clearance – standard valve clearance (IN: 0.3 mm {0.0118 in}, EX: 0.3 mm {0.0118 in})

  Standard valve clearance [Engine cold]

  IN: 0.27—0.33 mm {0.0107—0.0129 in}
  EX: 0.27—0.33 mm {0.0107—0.0129 in}

16. Align the timing marks on the crank pulley and the front cover, and then align the No.1 cylinder to the TDC.

am2zzw00004257

17. Install the intake and exhaust camshafts with the No.1 cylinder so that it is near TDC of the compression stroke.

18. Install the camshaft caps to the position shown in the figure, and temporarily tighten the No.2 and No.7 camshaft installation bolts.

19. Tighten the camshaft installation bolts in two or three steps uniformly in the order shown in the figure.

am2zzw00004258

  Tightening torque

  11.3—14.2 N·m {1.16—1.44 kgf·m, 8.4—10.4 ft·lbf}

20. Align the sprocket timing marks on the intake and exhaust camshafts so that they form a straight line in alignment with the upper horizontal surface of the cylinder head.

am2zzw00004259

21. Fix the camshaft using a wrench on the cast hexagon. Install the camshaft sprocket installation bolt.

  Tightening torque

  49.6—60.8 N·m {5.06—6.19 kgf·m, 36.6—44.8 ft·lbf}

22. Remove the M10 or M6 bolt holding the tensioner arm.

23. Verify that there is no slack in the timing chain, and then verify that the marks on the camshaft sprocket and the crank pulley are aligned.

24. Inspect the valve timing by rotating the crankshaft clockwise twice.

25. Install the engine front cover blind plug with a new washer. (Service Hole : 10 mm {0.39 in})

am2zzw00004422

  Tightening torque

  11.7—17.6 N·m {1.20—1.79 kgf·m, 8.7—12.9 ft·lbf}

26. Install the new engine front cover blind plug. (Service Hole : 7 mm {0.3 in})

am3zzw00006290

  Tightening torque

  3.0—6.0 N·m {31—61 kgf·cm, 26.6—53.1 in·lbf}

27. Install the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, ZY].)

28. Install the cylinder head cover. (See TIMING CHAIN REMOVAL/INSTALLATION [ZJ, ZY].)

29. Install the ventilation hose.

30. Install the ignition coils. (See IGNITION COIL REMOVAL/INSTALLATION [ZJ, ZY].)

31. Install the front tire (RH).