#
FRONT POWER WINDOW REGULATOR REMOVAL/INSTALLATION

id091200414600

1. Disconnect the negative battery cable.

2. Remove the front door glass.

3. Remove the front door speaker.

4. Remove the front power window motor.

5. Remove the nuts.

6. Insert hand through the front speaker installation hole, rotate the regulator drum housing in the direction shown in the figure and disengage the regulator drum housing from the door unit connection tabs.

7. Remove the front power window regulator from the speaker installation hole.

8. Install in the reverse order of removal.

  Caution

  • Make sure the cable does not unspool from the drum housing when installing.