#
SIMULATION FUNCTION [FN4A-EL]

id0502a1100800
• By using the WDS or equivalent, simulation items for input/output parts preset in the PCM can be optionally selected and operated regardless of PCM control conditions.

Simulation Item Table

X: Available

Simulation item | Applicable component | Unit/Condition | Operation | PCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
LPS | Pressure control solenoid control signal in PCM | % | X | X | 1AF 1AV
SSA/SS1 | Shift solenoid A control signal in PCM | % | X | X | 1AZ
SSB/SS2 | Shift solenoid B control signal in PCM | % | X | X | 1BH
SSC/SS3 | Shift solenoid C control signal in PCM | % | X | X | 1BD
SSD/ SS4 | Shift solenoid D control signal in PCM | On/Off | X | X | 1AJ
SSE_SS5 | Shift solenoid E control signal in PCM | On/Off | X | X | 1AR
test | - | On/Off | X | X | -