#
EVAPORATOR TEMPERATURE SENSOR INSPECTION

id074000801200

1. Set the temperature control at MAX COLD (Turn the left).

2. Turn the A/C switch.

3. Set the RECIRCULATE mode.

4. Close all doors and windows.

5. Wait for 5 min.

6. Remove the glove compartment.

7. Disconnect the evaporator temperature sensor.

8. Measure the temperature at the blower inlet.

9. Measure the resistance between terminals of the evaporator temperature sensor.

  • If the resistance is not as shown in the graph, replace the evaporator temperature sensor.