#
CIGARETTE LIGHTER REMOVAL/INSTALLATION

id092000803100

1. Disconnect the negative battery cable.

2. Remove the center panel module. (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

3. Remove the climate control unit.

4. Remove in the order indicated in the table.

1 | Cigarette lighter plug
2 | Socket (See Socket Removal Note) (See Socket Installation Note)
3 | Connector
4 | Ring (See Ring Removal Note)

5. Install in the reverse order of removal.

## Socket Removal Note

1. Put your hands inside the dashboard where the climate control unit was removed, and push the socket outward while pressing the ring protrusion using a tape-wrapped flathead screwdriver through the socket hole shown in the figure.

2. Push the socket outward by pressing the other ring protrusion using a tape-wrapped flathead screwdriver while the ring protrusion is released.

## Ring Removal Note

1. Put your hands inside the dashboard where the climate control unit was removed and pull the ring outward while pressing the tabs.

## Socket Installation Note

1. Install with the socket protrusion shown in the figure upward.