#
ABS HU/CM REMOVAL/INSTALLATION [APPLIED VIN (ASSUMED): JM0 DY10Y100 100001-108401, JM6 DY10*100 100001-109000]

id0413008014a5

  Caution

  • Do not drop the ABS HU/CM. Replace the ABS HU/CM if it is subjected to an impact.

1. Remove the battery and battery tray.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Brake pipe
2 | Connector (See Connector Removal Note) (See Connector Installation Note)
3 | ABS HU/CM component (See ABS HU/CM Component Removal/Installation Note)
4 | Bracket
5 | ABS CM
6 | ABS HU

## Connector Removal Note

1. Pull the connector cover up, and then remove the connector.

  Caution

  • If sand or other particles get into the connector cover, it may be difficult to remove. In order not to damage the connector, be careful not to use excessive force removing the cover.

## ABS HU/CM Component Removal/Installation Note

1. When removing/installing the ABS HU/CM component from/to the vehicle, attach a strip of protective tape on the ABS HU/CM component connector to prevent brake fluid from entering.

## Connector Installation Note

1. After connecting the connector, verify that the connector cover is completely locked.