#
BRAKES TECHNICAL DATA

id045000800100

Item | Specification
--- | ---
Brake fluid type | SAE J1703, FMVSS 116 DOT-3
Brake pedal height (reference value) | 208 mm {8.19 in}
Brake pedal play | 4.9-8.7 mm {0.2-0.3 in}
Brake pedal-to-floor clearance (Brake pedal when depressed at 588 N {60 kgf, 132 lbf}) | 79 mm {3.1 in} or more
Power brake unit fluid pressure when pedal depressed at 200 N {20.4 kgf, 44.9 lbf} | At 0 kPa {0 mmHg, 0 inHg}: 600 kPa {6.12 kgf/cm2, 87.0 psi} or more
Power brake unit fluid pressure when pedal depressed at 200 N {20.4 kgf, 44.9 lbf} | At 66.7 kPa {500 mmHg, 19.7 inHg}: 5,500 kPa {56.08 kgf/cm2, 797.5 psi} or more
Proportioning valve fluid pressure (without ABS) | Rear brake fluid pressure when front brake fluid pressure at 4,500 kPa {45.89 kgf/cm2, 652.5 psi}: 3,100 kPa {31.61 kgf/cm2, 449.5 psi} Rear brake fluid pressure when front brake fluid pressure at 10,000 kPa {101.97 kgf/cm2, 1,450 psi}: 4,750 kPa {48.44 kgf/cm2, 688.8 psi}
Front disc plate runout limit | 0.05 mm {0.002 in}
Minimum front disc plate thickness | 20 mm {0.79 in}
Minimum front disc plate thickness after machining using a brake lathe on-vehicle | 20.8 mm {0.82 in}
Minimum front disc pad thickness | 2.0 mm {0.079 in} min.
Minimum rear brake lining thickness | 1.0 mm {0.04 in}
Maximum rear brake drum inner diameter | 204.3 mm {8.043 in}
Parking brake lever stroke when pulled at 98 N {10 kgf, 22 lbf} | 3 notches or less