#
AIR FILTER INSPECTION

id071100800800

1. Remove the air filter.

2. Inspect the air filter.

  • If the air filter is damaged, excessively dirty, or foul smelling, replace the air filter.

  Note

  • The air filter cannot be reused by cleaning it with water or compressed air.
  • Replace the air filter at the following interval, depending on operating conditions.

Specs. | Type | Interval (year or km {miles})
--- | --- | ---
Europe (L.H.D. U.K.) specs. | Aldehyde, pollen, and a dust removal | 1 or 20,000 {12,500}
Pollen, and a dust removal | 2 or 40,000 {25,000}
General (L.H.D.) specs. | - | 1 or 20,000 {12,500}