#
EGR VALVE REMOVAL/INSTALLATION [WITH WU-TWC]

id0116008010b0

1. Remove the battery cover.

2. Disconnect the negative battery cable.

3. Disconnect the EGR valve connector.

4. Remove in the order indicated in the table.

1 | EGR pipe (Exhaust manifold side) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].)
2 | EGR valve

5. Replace the EGR valve gasket.

6. Install in the reverse order of removal.