#
BASIC INSPECTION [FN4A-EL]

id0503a1800300

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Perform the mechanical system test. (See MECHANICAL SYSTEM TEST [FN4A-EL].) Is mechanical system normal? | Yes | Go to next step.
No | Repair or replace any defective parts according to inspection result.
2 | Turn IG SW to ON. When selector lever is moved, does the selector illumination indicate synchronized position to lever location? Also, when other ranges are selected from N or P during idling, does vehicle moves within 1-2 seconds? | Yes | Go to next step.
No | Inspect selector lever and TR switch. Repair or replace defective areas. (See SELECTOR LEVER INSPECTION.) (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FN4A-EL].) If selector lever and TR switch are normal, go to next step.
3 | Inspect ATF color and condition. (See AUTOMATIC TRANSAXLE FLUID (ATF) INSPECTION [FN4A-EL].) Are ATF color and odor normal? | Yes | Go to next step.
No | Repair or replace any defective parts according to inspection result. Flush ATX and cooler line as necessary.
4 | Perform line pressure test. (See Line Pressure Test.) Is line pressure normal? | Yes | Go to next step.
No | Adjust accelerator cable as necessary. Repair or replace any defective parts according to inspection result.
5 | Perform stall test. (See Stall Test.) Is stall speed normal? | Yes | Go to next step.
No | Repair or replace any defective parts according to inspection result.
6 | Inspect the value at the following PIDs using the WDS or equivalent. (See PCM INSPECTION [WITHOUT WU-TWC].) (See PCM INSPECTION [WITH WU-TWC].) • TFT • TFT V • VPWR • TR • TR SENS • ECT • TCS • RPM • TP • TSS • VSS Is PID value normal? | Yes | Perform symptom troubleshooting and follow procedures.
No | Repair or replace any defective parts according to inspection result.