#
STEERING SHAFT INSPECTION

id061400800600

1. Inspect the column bearing for looseness and damage.

2. Verify that the measurement of the steering shaft as shown is the same as the specification.

  • Replace the steering shaft component if it is not within the specification.

Steering shaft length

  447 mm {17.6 in}

3. Inspect the tilt function in the following two ways.

  • If there is any malfunction, replace the steering shaft.
  (1) Verify that the tilt lever moves smoothly from the lock to the unlock position.
  (2) Verify that the steering shaft is fixed firmly when the tilt lever is locked.