#
AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [FN4A-EL]

id0517a1800600

  Warning

  • A hot transaxle and ATF can cause severe burns. Turn off the engine and wait until they are cool before changing the ATF.

1. Remove the oil dipstick.

2. Remove the oil drain plug and washer.

3. Drain the ATF into a container.

4. Install a new washer and the drain plug.

Tightening torque

  29.4-41.2 N·m
  {3.0-4.2 kgf·m, 21.7-30.3 ft·lbf}

5. Add the specified ATF until ATF level reaches lower notch of dipstick type of ATF through the oil filler tube.

ATF

  Type: ATF M-V
  Capacity (approx. quantity): 7.0 L {7.4 US qt, 6.1 lmp qt}

6. Ensure that the ATF level is in the HOT range (65 °C {149 °F}).

  • Add ATF to the specified level as necessary.